&soc {
	qcom,lpm-levels {
		compatible = "qcom,lpm-levels";
		reg = <0xfd91060 0x20>, <0xfd92060 0x20>;
		reg-names = "pwr", "perf";
		#address-cells = <1>;
		#size-cells = <0>;

		qcom,pm-cluster@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;
			idle-state-name = "L3";
			qcom,clstr-tmr-add = <1000>;
			qcom,psci-mode-shift = <4>;
			qcom,psci-mode-mask = <0xfff>;

			CLUSTER_WFI: qcom,pm-cluster-level@0 { /* D1 */
				reg = <0>;
				compatible = "arm,idle-state";
				idle-state-name = "l3-wfi";
				entry-latency-us = <660>;
				exit-latency-us = <600>;
				min-residency-us = <1260>;
				arm,psci-suspend-param = <0x10>;
				qcom,psci-mode = <0x1>;
			};

			CLUSTER_OFF: qcom,pm-cluster-level@1 { /* D4 */
				reg = <1>;
				compatible = "arm,idle-state";
				idle-state-name = "l3-pc";
				entry-latency-us = <2752>;
				exit-latency-us = <3048>;
				min-residency-us = <6118>;
				arm,psci-suspend-param = <0x40>;
				qcom,psci-mode = <0x4>;
				qcom,notify-rpm;
				qcom,min-child-idx = <2>;
				qcom,is-reset;
			};

			qcom,pm-cpu@0 {
				reg = <0>;
				#address-cells = <1>;
				#size-cells = <0>;
				qcom,psci-mode-shift = <0>;
				qcom,psci-mode-mask = <0xf>;
				label = "pwr";
				qcom,ref-stddev = <500>;
				qcom,tmr-add = <1000>;
				qcom,ref-premature-cnt = <1>;
				qcom,disable-ipi-prediction;
				qcom,cpu = <&CPU0 &CPU1 &CPU2 &CPU3 &CPU4
									&CPU5>;

				SLVR_WFI: qcom,pm-cpu-level@0 { /* C1 */
					reg = <0>;
					compatible = "arm,idle-state";
					idle-state-name = "wfi";
					entry-latency-us = <61>;
					exit-latency-us = <60>;
					min-residency-us = <121>;
					arm,psci-suspend-param = <0x1>;
					qcom,psci-cpu-mode = <0x1>;
				};

				SLVR_PC: qcom,pm-cpu-level@1 {  /* C3 */
					reg = <1>;
					compatible = "arm,idle-state";
					idle-state-name = "pc";
					entry-latency-us = <549>;
					exit-latency-us = <901>;
					min-residency-us = <1774>;
					qcom,psci-cpu-mode = <0x3>;
					arm,psci-suspend-param = <0x40000003>;
					local-timer-stop;
					qcom,is-reset;
					qcom,use-broadcast-timer;
				};

				SLVR_RAIL_OFF: qcom,pm-cpu-level@2 {  /* C4 */
					reg = <2>;
					compatible = "arm,idle-state";
					idle-state-name = "rail-pc";
					entry-latency-us = <702>;
					exit-latency-us = <915>;
					min-residency-us = <4001>;
					qcom,psci-cpu-mode = <0x4>;
					arm,psci-suspend-param = <0x40000004>;
					local-timer-stop;
					qcom,is-reset;
					qcom,use-broadcast-timer;
				};
			};

			qcom,pm-cpu@1 {
				reg = <1>;
				#address-cells = <1>;
				#size-cells = <0>;
				qcom,psci-mode-shift = <0>;
				qcom,psci-mode-mask = <0xf>;
				label = "perf";
				qcom,ref-stddev = <100>;
				qcom,tmr-add = <100>;
				qcom,ref-premature-cnt = <3>;
				qcom,cpu = <&CPU6 &CPU7>;

				GOLD_WFI: qcom,pm-cpu-level@0 { /* C1 */
					reg = <0>;
					idle-state-name = "wfi";
					compatible = "arm,idle-state";
					entry-latency-us = <55>;
					exit-latency-us = <66>;
					min-residency-us = <121>;
					qcom,psci-cpu-mode = <0x1>;
					arm,psci-suspend-param = <0x1>;
				};

				GOLD_PC: qcom,pm-cpu-level@1 {  /* C3 */
					reg = <1>;
					compatible = "arm,idle-state";
					idle-state-name = "pc";
					entry-latency-us = <523>;
					exit-latency-us = <1244>;
					min-residency-us = <2207>;
					arm,psci-suspend-param = <0x40000003>;
					local-timer-stop;
					qcom,psci-cpu-mode = <0x3>;
					qcom,is-reset;
					qcom,use-broadcast-timer;
				};

				GOLD_RAIL_OFF: qcom,pm-cpu-level@2 {  /* C4 */
					reg = <2>;
					compatible = "arm,idle-state";
					idle-state-name = "rail-pc";
					entry-latency-us = <526>;
					exit-latency-us = <1854>;
					min-residency-us = <5555>;
					arm,psci-suspend-param = <0x40000004>;
					local-timer-stop;
					qcom,psci-cpu-mode = <0x4>;
					qcom,is-reset;
					qcom,use-broadcast-timer;
				};
			};
		};
	};

	rpm_sleep_stats: soc-sleep-stats@4690000 {
		compatible = "qcom,rpm-sleep-stats";
		reg = <0x04690000 0x400>;
	};

	qcom,rpm-master-stats@45f0150 {
		compatible = "qcom,rpm-master-stats";
		reg = <0x45f0150 0x5000>;
		qcom,masters = "APSS", "MPSS", "ADSP", "CDSP", "TZ";
		qcom,master-stats-version = <2>;
		qcom,master-offset = <4096>;
	};

};
