&mdss_mdp {
	dsi_sw43404_amoled_fhd_plus_cmd: qcom,mdss_dsi_sw43404_fhd_plus_cmd {
		qcom,mdss-dsi-panel-name =
		  "sw43404 amoled boe fhd+ panel with DSC";
		qcom,mdss-dsi-panel-type = "dsi_cmd_mode";
		qcom,mdss-dsi-panel-physical-type = "oled";
		qcom,dsi-ctrl-num = <0>;
		qcom,dsi-phy-num = <0>;

		qcom,mdss-dsi-virtual-channel-id = <0>;
		qcom,mdss-dsi-stream = <0>;
		qcom,mdss-dsi-bpp = <24>;
		qcom,mdss-dsi-color-order = "rgb_swap_rgb";
		qcom,mdss-dsi-underflow-color = <0xff>;
		qcom,mdss-dsi-border-color = <0>;

		qcom,mdss-dsi-traffic-mode = "non_burst_sync_event";
		qcom,mdss-dsi-lane-map = "lane_map_0123";
		qcom,mdss-dsi-bllp-eof-power-mode;
		qcom,mdss-dsi-bllp-power-mode;
		qcom,mdss-dsi-lane-0-state;
		qcom,mdss-dsi-lane-1-state;
		qcom,mdss-dsi-lane-2-state;
		qcom,mdss-dsi-lane-3-state;
		qcom,mdss-dsi-dma-trigger = "trigger_sw";
		qcom,mdss-dsi-mdp-trigger = "none";
		qcom,mdss-dsi-reset-sequence = <1 10>, <0 10>, <1 10>;
		qcom,mdss-dsi-te-pin-select = <1>;
		qcom,mdss-dsi-wr-mem-start = <0x2c>;
		qcom,mdss-dsi-wr-mem-continue = <0x3c>;
		qcom,mdss-dsi-te-dcs-command = <1>;
		qcom,mdss-dsi-te-check-enable;
		qcom,mdss-dsi-te-using-te-pin;
		qcom,mdss-pan-physical-width-dimension = <68>;
		qcom,mdss-pan-physical-height-dimension = <138>;
		qcom,mdss-dsi-panel-hdr-enabled;
		qcom,mdss-dsi-panel-hdr-color-primaries = <14500 15500 32000
			17000 15500 30000 8000 3000>;
		qcom,mdss-dsi-panel-peak-brightness = <4200000>;
		qcom,mdss-dsi-panel-blackness-level = <3230>;

		qcom,mdss-dsi-display-timings {
			timing@0 {
				qcom,mdss-dsi-panel-framerate = <60>;
				qcom,mdss-dsi-panel-width = <1080>;
				qcom,mdss-dsi-panel-height = <2160>;
				qcom,mdss-dsi-h-front-porch = <160>;
				qcom,mdss-dsi-h-back-porch = <72>;
				qcom,mdss-dsi-h-pulse-width = <16>;
				qcom,mdss-dsi-h-sync-skew = <0>;
				qcom,mdss-dsi-h-sync-pulse = <0>;
				qcom,mdss-dsi-v-back-porch = <8>;
				qcom,mdss-dsi-v-front-porch = <8>;
				qcom,mdss-dsi-v-pulse-width = <1>;
				qcom,mdss-dsi-h-left-border = <0>;
				qcom,mdss-dsi-h-right-border = <0>;
				qcom,mdss-dsi-v-top-border = <0>;
				qcom,mdss-dsi-v-bottom-border = <0>;
				qcom,mdss-dsi-panel-jitter = <0x3 0x1>;
				qcom,mdss-dsi-on-command = [
				  39 01 00 00 00 00 03 b0 a5 00
				  07 01 00 00 00 00 02 01 00
				  0a 01 00 00 00 00 80 11 00 00 89 30 80
				     08 70 04 38 02 1c 02 1c 02 1c 02 00
				     02 0e 00 20 34 29 00 07 00 0C 00 2e
				     00 31 18 00 10 F0 03 0C 20 00 06 0B
				     0B 33 0E 1C 2A 38 46 54 62 69 70 77
				     79 7B 7D 7E 01 02 01 00 09 40 09 BE
				     19 FC 19 FA 19 F8 1A 38 1A 78 1A B6
				     2A F6 2B 34 2B 74 3B 74 6B F4 00 00
				     00 00 00 00 00 00 00 00 00 00 00 00
				     00 00 00 00 00 00 00 00 00 00 00 00
				     00 00 00 00 00 00 00 00 00 00 00 00
				     00 00
				  39 01 00 00 00 00 03 b0 a5 00
				  15 01 00 00 00 00 02 5e 10
				  39 01 00 00 00 00 06 b9 bf 11 40 00 30
				  39 01 00 00 00 00 09 F8 00 08 10 08 2D
					   00 00 2D
				  15 01 00 00 00 00 02 55 08
				  05 01 00 00 1e 00 02 11 00
				  15 01 00 00 78 00 02 3d 01
				  39 01 00 00 00 00 03 b0 a5 00
				  05 01 00 00 78 00 02 35 00
				  05 01 00 00 3c 00 02 29 00
				];
				qcom,mdss-dsi-off-command = [
					05 01 00 00 14 00 02 28 00
					05 01 00 00 78 00 02 10 00];
				qcom,mdss-dsi-on-command-state = "dsi_lp_mode";
				qcom,mdss-dsi-off-command-state = "dsi_hs_mode";
				qcom,compression-mode = "dsc";
				qcom,mdss-dsc-slice-height = <270>;
				qcom,mdss-dsc-slice-width = <540>;
				qcom,mdss-dsc-slice-per-pkt = <1>;
				qcom,mdss-dsc-bit-per-component = <8>;
				qcom,mdss-dsc-bit-per-pixel = <8>;
				qcom,mdss-dsc-block-prediction-enable;
			};
		};
	};
};
